Output of erosions, dilations and re-thresholding tab

Output of thresholding

tab

itk::MIDASMorphologicalSegmentor

LargestConnectedComponentFilter

Input "Edits" image

(binary)

(connection breaker)

Input image

(grey scale)

Input "Additions" image

(binary)

itk::MIDASRethresholdingFilter

itk::MIDASConditionalDilationFilter

itk::MIDASConditionalErosionFilter

itk::MIDASMaskByRegionImageFilter

(axial cut-off)

itk::BinaryThresholdImageFilter